{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":2,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":7,"rows_kept":5,"merged":[[0,0,0,6],[4,0,4,6]],"flags":["formulas_cached_only"]}
["金审学院学生公寓座椅采购清单"]
["序号","名称","图片","规格尺寸","材料说明","使用场所","数量需求（把）"]
[1,"公寓椅A",null,"宽480*高460（含靠背800）深510","1.椅脚直径25mm-35mm锥形圆柱体，椅面下边四周带加固飞边，宽度35mm，椅面采用人体工程学，体感舒适，靠背带连体镂空，镂空尺寸250mm*200mm；（尺寸可调）                                                             2.材料采用PP工程塑料，注塑一体成型，内含高弹力尼龙，确保椅面经长时间不开裂，不变性，韧性强；                                                       3.颜色为草绿麻面色，色泽均匀，无露色、无色差；  （颜色可选）                                 4.椅面承载不低于300公斤，椅脚摆动不低于150公斤，靠背摇摆不低于150公斤；                                                                                   5.靠背最大摆动15度，不易开裂、不易断裂；                                          6.椅脚内带直径16mm*1.5mm厚镀锌钢管，底部带消音防滑套脚；                               7.椅子质保9年，9年内（除人为原因）无条件维修，响应时间24小时，修复时间48小时。","1、6号楼、专家楼",642]
[2,"公寓椅B",null,"宽420*深415*高420（含靠背820）","1.椅脚底部20mm*25mm，椅脚上部20mm*60mm扁圆锥形体，椅面下边四周带加固飞边，宽度50mm-70mm，椅面采用人体工程学，体感舒适；（尺寸可调)                                                             2.材料采用PP工程塑料，注塑一体成型，内含高弹力尼龙，确保椅面经长时间不开裂，不变性，韧性强；                                                       3.颜色为深蓝色，色泽均匀，无露色、无色差； （颜色可选）                       4.椅面和靠背及椅架可拆分，螺丝固定；                                   5.椅面承载不低于300公斤，椅脚摆动不低于150公斤，靠背摇摆不低于150公斤；                                                                                   6.靠背最大摆动15度，不易开裂、不易断裂；                                          7.底部带消音防滑套脚；                                              8.椅子质保9年，9年内（除人为原因）无条件维修，响应时间24小时，修复时间48小时。","2、3号楼",3886]
["注：最终采购数量以采购方实际需求为准"]