{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["A更换","B维修 ","C维修 ","报价表"],"read":"whole","date_system":"1900"}

{"sheet":"A更换","index":0,"n_rows":19,"n_cols":10,"rows_kept":19,"merged":[[0,0,0,9],[1,0,2,0],[1,1,1,2],[1,3,2,3],[1,4,1,7],[1,8,2,8],[1,9,2,9],[14,9,16,9],[17,0,17,2]]}
["卫生间内门及隔断等需作全部更换处理情况统计（A类）"]
["序号","位置",null,"门樘数","破损情况",{"$nulls":3},"维修建议","备注"]
[null,"楼宇名称","具体方位",null,"门","隔断","内锁","铰链（含地面固定）"]
[1,"B教学楼","西南二楼女",11,2,1,2,"腐烂","A"]
[2,"B教学楼","西南四楼女",11,0,1,1,"腐烂","A"]
[3,"B教学楼","中西二楼男",6,2,1,3,"腐烂","A"]
[4,"B教学楼","中西三楼男",6,2,1,3,"腐烂","A"]
[5,"B教学楼","中西三楼女",11,1,1,6,"腐烂","A"]
[6,"B教学楼","西北三楼男",6,1,1,3,1,"A"]
[7,"体艺楼","一楼东南角女厕",4,4,1,4,0,"A"]
[8,"体艺楼","一楼东南角男厕",4,4,3,4,"腐烂","A"]
[9,"体艺楼","一楼西南角男厕",3,3,3,3,"腐烂","A"]
[10,"体艺楼","一楼西北角女厕",4,4,1,4,0,"A"]
[11,"体艺楼","三楼西南角男厕",3,3,3,3,"腐烂","A"]
[12,"体艺楼","三楼西北角女厕",3,0,3,0,"腐烂","A","换下的门调作二层使用"]
[13,"体艺楼","三楼东南角女厕",3,1,0,1,0,"A"]
[14,"体艺楼","三楼东南角男厕",3,1,0,1,0,"A"]
["合计",null,null,{"$f":"SUM(D4:D17)","v":78},{"$f":"SUM(E4:E17)","v":28},{"$f":"SUM(F4:F17)","v":20},{"$f":"SUM(G4:G17)","v":38},null,14]
[{"$nulls":5},"统计人：",null,null,"时间"]

{"sheet":"B维修 ","index":1,"n_rows":27,"n_cols":10,"rows_kept":27,"merged":[[0,0,0,9],[1,0,2,0],[1,1,1,2],[1,3,2,3],[1,4,1,7],[1,8,2,8],[1,9,2,9],[3,9,15,9],[25,0,25,2]]}
["卫生间内门（含迎面板、拉条及内锁）需作更换处理情况统计（B类）"]
["序号","位置",null,"门樘数","破损情况",{"$nulls":3},"维修建议","备注"]
[null,"楼宇名称","具体方位",null,"门","隔断","内锁","铰链（含地面固定）"]
[1,"B教学楼","一楼东男",4,4,0,4,0,"B","B教学楼厕所内门及迎面板或迎面板与门相连处破损严重，无法修复。"]
[2,"B教学楼","一楼东女",4,4,0,4,0,"B"]
[3,"B教学楼","东南二楼男",4,0,0,2,0,"B"]
[4,"B教学楼","东南二楼女",4,4,0,0,0,"B"]
[5,"B教学楼","东南三楼女",4,1,0,0,0,"B"]
[6,"B教学楼","东北二楼女",4,1,0,2,null,"B"]
[7,"B教学楼","西南四楼男",6,1,0,4,0,"B"]
[8,"B教学楼","中西一楼女",11,2,0,3,0,"B"]
[9,"B教学楼","中西二楼女",11,3,0,0,0,"B"]
[10,"B教学楼","中西四楼男",6,1,0,0,0,"B"]
[11,"B教学楼","西北二楼男",6,5,0,1,0,"B"]
[12,"B教学楼","西北二楼女",11,3,0,0,0,"B"]
[13,"B教学楼","西北三楼女",11,1,0,0,0,"B"]
[14,"体艺楼","二楼西北角女厕",3,3,0,0,0,"B","门变形"]
[15,"体艺楼","二楼东南角男厕",4,1,0,1,0,"B","门变形"]
[16,"T南","一楼南男厕",5,5,1,5,0,"B","隔断底部有破损，不影响使用"]
[17,"T南","一楼南女厕",8,7,2,5,0,"B","同上"]
[18,"T南","一楼东男厕",4,4,0,4,0,"B"]
[19,"T南","一楼东女厕",8,8,0,8,0,"B"]
[20,"T南","二楼南男厕",5,5,1,5,0,"B"]
[21,"T南","二楼南女厕",8,8,0,6,0,"B"]
[22,"T南","二楼东女厕",8,3,0,3,0,"B","一处迎面板及贴边全坏"]
["合计",null,null,{"$f":"SUM(D4:D25)","v":139},{"$f":"SUM(E4:E25)","v":74},10,{"$f":"SUM(G4:G25)","v":57},{"$f":"SUM(H4:H25)","v":0},23]
[{"$nulls":5},"统计人：",null,null,"时间"]

{"sheet":"C维修 ","index":2,"n_rows":33,"n_cols":10,"rows_kept":33,"merged":[[0,0,0,9],[1,0,2,0],[1,1,1,2],[1,3,2,3],[1,4,1,7],[1,8,2,8],[1,9,2,9],[3,9,16,9],[17,9,26,9],[27,9,30,9],[31,0,31,2]]}
["卫生间内门、内锁等需作局部维修处理情况统计（C类）"]
["序号","位置",null,"门樘数","破损情况",{"$nulls":3},"维修建议","备注"]
[null,"楼宇名称","具体方位",null,"门","隔断","内锁","铰链（含地面固定）"]
[1,"A教学楼","一楼西女厕",5,1,0,1,0,"C","迎面板及门及门上横条均为铝合金包边，只需更换门、内锁及连接的铰链，建议做维修处理"]
[2,"A教学楼","一楼西男厕",5,3,0,4,0,"C"]
[3,"A教学楼","二楼西男厕",5,4,0,4,0,"C"]
[4,"A教学楼","二楼西女厕",5,3,0,3,0,"C"]
[5,"A教学楼","三楼西男厕",5,2,0,2,0,"C"]
[6,"A教学楼","三楼西女厕",5,4,0,4,0,"C"]
[7,"A教学楼","四楼东男厕",5,5,0,5,0,"C"]
[8,"A教学楼","四楼东女厕",5,4,0,4,0,"C"]
[9,"A教学楼","四楼西男厕",5,2,0,3,0,"C"]
[10,"A教学楼","四楼西女厕",5,1,0,1,0,"C"]
[11,"A教学楼","五楼东男厕",4,4,0,4,0,"C"]
[12,"A教学楼","五楼东女厕",4,2,0,2,0,"C"]
[13,"A教学楼","五楼西男厕",5,4,0,4,0,"C"]
[14,"A教学楼","五楼西女厕",5,1,0,1,0,"C"]
[15,"B教学楼","东南三楼男",4,0,0,3,0,"C","内锁及搭扣损坏（有明细）"]
[16,"B教学楼","东南四楼男",4,0,0,2,0,"C"]
[17,"B教学楼","东北二楼男",4,0,0,1,null,"C"]
[18,"B教学楼","西南三楼男",6,0,0,4,0,"C"]
[19,"B教学楼","西南三楼女",11,0,0,1,0,"C"]
[20,"B教学楼","中西一楼男",6,0,0,4,0,"C"]
[21,"B教学楼","中西四楼女",11,0,0,1,0,"C"]
[22,"T北","一至四楼",null,0,0,8,0,"C"]
[23,"信息楼","南楼",{"$nulls":3},11,null,"C"]
[24,"信息楼","北楼",{"$nulls":3},8,null,"C"]
[25,"T南","三楼南男厕",3,0,0,0,0,"C","换门贴边（挡内锁用）及内锁\n\n"]
[26,"T南","三楼南女厕",3,0,0,1,0,"C"]
[27,"T南","四楼南男厕",3,0,0,0,0,"C"]
[28,"T南","四楼南女厕",4,0,0,0,0,"C"]
["合计",null,null,139,{"$f":"SUM(E4:E25)","v":40},0,{"$f":"SUM(G4:G25)","v":66},0,32]
[{"$nulls":5},"统计人：",null,null,"时间"]

{"sheet":"报价表","index":3,"n_rows":19,"n_cols":8,"rows_kept":19,"merged":[[0,0,0,7],[1,0,1,1],[2,0,3,0],[2,1,3,1],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[4,1,4,5],[7,0,7,1],[9,0,9,1],[10,0,11,0],[10,1,11,1],[10,3,11,3],[10,4,11,4],[10,5,11,5],[10,6,11,6],[10,7,11,7],[12,1,12,5],[15,0,15,1],[17,0,17,7],[18,0,18,7]]}
["教学楼、体艺楼维修卫生间门及隔断报价表"]
["投标单位名称："]
["更换名称","更换说明","门及隔板","隔断","内锁","铰链、底座","其他","合计"]
[null,null,"抗倍特"]
["A类更换","78个蹲位全套换"]
["B类更换","139个蹲位厕所迎面板和厕所门及相关配件全部更换"]
["C类更换","迎面板及门及门上横条均为铝合金包边，只需更换门、内锁及连接的铰链，门40个，内锁66个,15个门边压条"]
["合计"]
[]
["投标单位名称："]
["更换名称","更换说明","门及隔板","隔断","内锁","铰链、底座","其他","合计"]
[null,null,"多层饰面夹层板"]
["A类更换","78个蹲位全套换"]
["B类更换","139个蹲位厕所迎面板和厕所门及相关配件全部更换"]
["C类更换","迎面板及门及门上横条均为铝合金包边，只需更换门、内锁及连接的铰链，门40个，内锁66个,15个门边压条"]
["合计"]
[]
["备注：1、报价中应含拆除下来的可利用门板及在C类中的使用情况。"]
["      2、同一厕所内的面板需保持一致。"]