{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":7,"rows_kept":9,"merged":[[0,0,0,6],[1,0,1,6],[4,0,4,4],[5,0,5,6],[6,0,6,6],[7,0,7,6],[8,0,8,6],[9,0,9,6]]}
[]
["南京审计大学金审学院9号学生宿舍楼及食堂勘察清单报价一览表"]
["序号","项目名称","特征描述","长度\n（m）","单价\n（元/m）","合价（元）","备注"]
[1,"地质详勘","1.结合设计单位要求，根据场地实际土层分布，调整布孔，场地周边应补充供基坑支护设计要求的勘探点，地勘部门可根据相关规范要求适当调整勘察点间距及勘探孔深度。\n2.查明拟建筑物范围内各层岩土的类别，结构、厚度、工程特性。\n3.了解场地内是否有暗浜、池塘、池、井等，查明不良地质作用的成因，类型、分布范围、发展趋势及危害程度。\n4.划分场地类别，分析地震效应情况，判定饱和砂土和饱和粉土的地震  情况，并计算其液化指数。\n5.查明地下水的埋设条件，评价场地内水，土对砼、砼中钢筋的腐蚀性。\n6.对可能采取的基础型式提出建议，提供基础设计所需的岩土技术参数。若为桩基础，须查明并提供相关参数。\n7.提出基础工程设计，施工中应注意的问题。\n8.提供满足地基基础设计要求的岩土工程勘察报告。\n9.未尽事宜按现行《岩土工程勘察规范》（GB50021-2017）等规范执行\n10.勘察设计要求见图纸及总说明，未说明之处，均按国家现行规范及本地区的规范执行，所提供的成果应满足规范的要求。 \n11.场地现状、土质、钻探深度、措施费、规费、税金等综合考虑在单价中。",{"$f":"17*20+10*25","v":590}]
["合计（元）"]
["注： 1、投标申请人应按照国家有关工程建设标准强制性条文和建设部有关标准、规范、规程、办法、示例等要求的内容和深度， 开展本项目的勘察工作，并将勘察费计入相应的报价项目中。投标申请人的报价，应包括测量、勘察以及专题研究等为完成本工程施工及竣工验收全过程的一切费用， 包括按合同规定应完成的勘察费和后续服务费。"]
["    2、工作内容包括但不仅限于上述工作内容，投标人可在满足设计要求的前提下自行增加， 费用含在投标报价内，结算时不调整。"]
["    3、本报价为完成招标文件全部工作内容的总报价，合同一经签订，价格即为固定总价，除不可抗力外，单价不得调整。"]
[" 4、发票必须提供专用增值税发票。"]